**STRUCTURAL PALLET RACKING**

|  |  |
| --- | --- |
| Completed by: |  |
| Company: |  |
| Email Address: |  |

|  |  |
| --- | --- |
| **Number of runs** |  |
| **Number of bays per run** |  |
| **Clear entry - left to right (mm)** *– max 3,900mm* |  |
| **Capacity per level (kg)** *– max 3,000kgs beam load  max 15,000kgs per frame* |  |
| **Height (mm)** *– max 5,000mm* |  |
| **Rack depth** *– max 1,100mm* |  |
| **Number of beam levels** |  |
| **Specific vertical clearance between beams? (mm)** *Adjustment pitch is 100mm* |  |
| **Finish** *Galvanised bracing fitted with all finishes* | Painted  *Black (Standard)*  *Other (Please specify):*  Galvanised |
| **Delivery Location** |  |
| **E/O for installation** | Yes  No |

**Product Details:**

|  |
| --- |
| Weight, each (kg): |

**A:**

A

B

C

A

C

B

**B:**

A

C

B

**C:**

**Extras:**

|  |  |
| --- | --- |
| Pallet Support Bars  Fork Entry Bars  Coil Cradles  Pallet Backstops | Timber Decking  Steel Mesh Decking |

**Notes:**